Sender process(rt\_srv):

1.Get data from local app, calculate the deliveryTime then store it into the window and send it to the Receiver. (deliveryTime = sendTS+ baseDelta + lantency Window)

2.Check whether we should shift the window.

If (packet delivery time < present time+ base\_Delta) then we shift otherwise, do nothing.

3.Receive the ACK packet from receiver and update the Base\_Delta, RTT.

Send the ACKACK packet And check whether we have NACK and resend packet if its( delivery time > present time + base\_Delta)

When resending the Nack, we replace sendTS with present time,but keep the same delivery time.

Receiver process(rt\_rcv): The receiver has three main responsibilities.

The first responsibility is Receiving the packet from Sender.

There could be two types of packet.

1. Data Packet: Check whether we already had the packet. If not, check whether the delivery time is not expired. If not write it into our buffer.
2. ACKACK Packet: the receiver gets packets and adjust the Base\_delta and Drift.

RTT =(recvTime2– recvTime1) = (ACKACK\_TS- Send\_TS)

Base\_delta = ½ RTT + clock\_diff= recvTime2 – ACKACK\_TS = recvTime1- Send\_TS

The second responsibility is sending the ACK and NACKs to sender.

The third responsibility is Delivering the packet on Delivery Time.

Data Structure of Sender

2d array Buffer Window

Time Base\_Delta

Time RTT

Time clock\_diff /\*Optional\*/

Time lantencywindow

Data Structure of Receiver

2d array Latency Window

Time Base\_Delta

Time RTT

Time clock\_diff /\*Optional\*/

array to store recent 50 RTT /\*aim for updating RTT\*/

array to store recent 50 Base\_Delta /\* aim for updating Base\_Delta\*/

Data Structure of Message

/\* 0-> Sender sends data to Receiver

1->Sender sends ACKACK

2->Sender Receive ACK from Receiver\*/

Type

Seq /\* Sequence number of Data Packet\*/

Delivery Time /\* The delivery time of data\*/

DATA

ACK

NACK

ACKACK /\* ACK of ACK\*/

Send\_TS /\*Send time of packet

It could change when we resend the Packet\*/

Receive1\_TS /\*First time receiver receives the packet \*/

ACKACK\_TS /\*The time when sender gets the ACK \*/

Receive2\_TS /\* No need, it is the time when receiver gets ACKACK \*/

Base\_Delta /\*Measure of ½ RTT+ clock \_diff\*/

RTT /\*Round trip time between sender and receiver\*/

Question1: how big will the window be ? lantency window time.

Question2: When updating the Base\_Delta, how to deal with the delivery time of the packet already in the latency window.

Text

Description automatically generated with medium confidence

1.Sender

Initial { type:0 | seq | read data | Delivery Time |

sendTS| }

{ACK, NACK,ACKACK = -1, Base\_Delta = -1, Drift = -1

Receive1\_TS,ACKACK\_TS = NULL}

2.Receiver

Take Receive1\_TS

Type set to 1

Find Nack

Send ACK= seq

Put Updated Base\_Delta, Drift

3.Sender

Take ACKACK\_TS

Type set to 2

Adjust Base\_Delta and Drift

4.Receiver

Get ACKACK\_TS,

calculate new RTT

new Base\_Delta